Excelsior V6 PLUS In-Wall Touchpanel 18,5 inch

|  |  |
| --- | --- |
| Technical Specifications | |
| Hardware | * CPU: Intel Core i5 8265U * Main memory: 16 GB RAM * Hard disk storage: 240 GB SSD * Power supply: 24V / 3,8A DIN rail mount |
| Interface | * USB port: 4xUSB 3.1, 1xUSB3.1 Type-C * LAN port : 2xRJ45 LAN Gigabit * Video port: 1xHDMI, 1xDP * Audio port: 1x Line-out |
| Display | * Size: 18,5 inch screen diagonal * Resolution: 1920 x 1080 pixels (Full HD) * Aspect ratio: 16 : 9 * Touch: projected capacitive touchscreen (PCT / PCAP) * Frame color: black / white |
| Audio | * Speakers: 2x integrated speakers (2W each) * Microphone: integrated microphone (for noise cancelling:  Voice Performance brick) |
| Measurements | * Display size: 230 mm x 410 mm (H x W) * Total size: 313 x 493 x 75 mm (H x W x D) * Weight: 3,5 kg |

|  |  |
| --- | --- |
| Software | |
| Operating system | * Windows 10 IoT Enterprise 2019 LTSC |
| Additional software | BasisModul (HC-Navigation + HC-Camviewer)  RadioModul  HC-SipPhone  HC-Browser  HC-PictureViewer  TV-Modul |

|  |  |
| --- | --- |
| Additional equipment | |
| Necessary | * Wallbox * Flush mount wallbox |
| Optional | Presence detector brick  Voice Performance brick   Camera brick (5 mega pixel)  Backup & Recovery USB Stick 64 GB |

Serial number:Klicken Sie hier, um Text einzugeben.