Excelsior V6 Wallmount Touchpanel 18,5 inch

|  |
| --- |
| Technical Specifications |
| Hardware | * CPU: Intel Core i5 8265U
* Main memory: 8 GB RAM
* Hard disk storage: 120 GB SSD
* Power supply: 24V / 3,8A DIN rail mount
 |
| Interface | * USB Port: 4xUSB 3.0, 2xUSB 2.0
* LAN Port : 2xRJ45 LAN Gigabit
* Video Port: 1xHDMI, 1xDP
* Audio Port: 1x Line-out
 |
| Display | * Size: 15 inch screen diagonal
* Resolution: 1920 x 1080 pixels (Full HD)
* Aspect ratio: 16 : 9
* Touch: projected capacitive touch (PCT / PCAP)
* Frame color: black / white
 |
| Audio | * Speakers: 2 x integrated speakers (je 2 W)
* Mikrophone: integrated microphone (for noise cancelling: Voice Performance brick)
 |
| Measurements | * Display size: 230 mm x 410 mm (H x W)
* Total size: 313 x 493 x 52 mm (H x W x D)
* Gewicht: 3,5 kg
 |

|  |
| --- |
| Software |
| Operating system | * Windows 10 IoT Enterprise 2019 LTSC
 |
| Additional software |  [ ]  BasisModul (HC-Navigation + HC-Camviewer) [ ]  RadioModul [ ]  HC-SipPhone [ ]  HC-Browser [ ]  HC-PictureViewer [ ]  TV-Modul |

|  |
| --- |
| Zubehör |
| Necessary | * Wallbox
* Flushmount wallbox
 |
| Optional |  [ ]  Presence detector brick [ ]  Voice Performance brick [ ]  Camera brick (5 mega pixel) [ ]  Backup & Recovery USB Stick 64 GB |

 Serial number:Klicken Sie hier, um Text einzugeben.