Levior In-Wall Touchpanel 21,5 inch

|  |
| --- |
| Technical Specifications |
| Hardware | * CPU: Intel J3455 Quad Core
* Main memory: 8 GB RAM
* Hard disk storage: 120 GB SSD
* Power supply: 15V / 4A DIN rail mount
 |
| Interaface | * USB port: 4xUSB 3.0
* LAN port : 2xRJ45 LAN Gigabit
* Video port: 2xHDMI
* Audio port: 1x Line-out
 |
| Display | * Size: 21,5 inch screen diagonal
* Resolution: 1920 x 1080 pixels (Full HD)
* Aspect ratio: 16 : 9
* Touch: projected capacitive touchscreen (PCT / PCAP)
* Frame color: black / white
 |
| Measurements | * Display size: 268 mm x 476 mm (H x W)
* Total size: 349 x 558 x 75 mm (H x W x D)
* Weight: 3,5 kg
 |

|  |
| --- |
| Software |
| Operating system | * Windows 10 IoT Enterprise 2019 LTSC
 |
| Additional software |  [ ]  BasisModul (HC-Navigation + HC-Camviewer) [ ]  HC-Browser [ ]  HC-PictureViewer |

|  |
| --- |
| Additional equipment |
| Necessary | * Wallbox
* Flush mount wallbox
 |
| Optional |  [ ]  Presence detector brick  [ ]  Camera brick (5 mega pixel) [ ]  Backup & Recovery USB Stick 64 GB |

 Serial number:Klicken Sie hier, um Text einzugeben.